**Measurements required for bay windows**

**Single Bend**

**A**

**B**

**C**

Measurements required:

A-B

B-C

A-C

Angle at B - approx

This track will be supplied with 2 equal legs to the longest measurement

**2 Bend Square Bay**

Measurements required:

**A**

**B**

**C**

**D**

A-B, A-C, A-D

B-C, B-D

C-D

Angles at B and C - approx

**Please state if this is track size or wall size, Which brackets are you using?**

**2 Bend Square Bay with returns**

Measurements required:

**A**

**B**

**C**

**D**

**X**

**Y**

A-B, A-C, A-D, A-X

B-C, B-D

C-D, D-Y

Angles at, A B C and D - approx

**Please state if this is track size or wall size, Which brackets are you using?**

**2 Bend Splay Bay**

Measurements required:

**A**

**B**

**C**

**D**

A-B, A-C, A-D

B-C, B-D

C-D

Angles at B and C –

**Please state if this is track size or wall size, Which brackets are you using?**

**2 Bend Splay Bay with returns**

Measurements required:

**A**

**B**

**C**

**D**

**Y**

**X**

A-B, A-C, A-D, A-X

B-C, B-D

C-D, D-Y

Angles at A B C & D

**Please state if this is track size or wall size, Which brackets are you using?**

**4 Bend Splay Bay**

Measurements required:

**A**

**B**

**C**

**D**

**E**

**F**

A-B, A-C, A-D, A-E, A-F

B-C, B-D, B-E, B-F

C-D, C-E, C-F

D-E, D-F

E-F

Angles at B,C D and E

**Please state if this is track size or wall size, Which brackets are you using?**

**4 Bend Splay Bay with returns**

Measurements required:

**A**

**B**

**C**

**D**

**E**

**F**

**X**

**B**

A-B, A-C, A-D, A-E, A-F

B-C, B-D, B-E, B-F

C-D, C-E, C-F

D-E, D-F

E-F

A-X, F-Y

Angles at A B,C D E and F

**Please state if this is track size or wall size, Which brackets are you using?**

**D**

**5 Bend “50p-bit” Bay**

Measurements required:

**A**

**B**

**C**

**E**

**F**

**G**

A-B, A-C, A-D, A-E, A-F, A-G

B-C, B-D, B-E, B-F,B-G

C-D, C-E, C-F, C-G

D-E, D-F,D-G

E-F, E-G,

F-G

Angles at B,C D E and F

**Please state if this is track size or wall size, Which brackets are you using?**

**This bay can also have returns if required as in previous bays**

**Bow Windows**

It is also possible to curve or even arch the track and combine the curve with bends straights and other curves, even a complete circle. For all of these special shapes, a life-size template would be required.